DELIVERED JUNE 2014
TRANSMISSOMETER DATA README FILE - JUNE 2014
This data package contains level-1 hourly transmissometer-based visibility data from the  remaining transmissometer site (listed below) in the IMPROVE visibility monitoring network.  This transmissometer site is operated by USDA-FS. The data included are from 1/1/13 through 12/31/13.  There are a total of 4 transmissometer level-1 data files included.  As with all level-1 transmissometer data, careful attention should be paid to the validity interference codes, which indicate a variety of uncertainties in the processed measurements.  
DATA FILE FORMAT KEY

The data file format key for all transmissometer data files is included in this folder and is available in:

· MS Word format
 
  (transkeyNov2003.doc)

· Adobe Acrobat format
  (transkeyNov2003.pdf)

· Text only

 
  (transkeyNov2003.txt)

FILE NAMING CONVENTIONS

Quarterly data files are named XXXXX_T1W.YYS, where XXXXX is the site abbreviation, YY is the year, and S is the calendar season:

1. =
Winter
   
(January, February, and March)

2. =
Spring 
  
(April, May, and June)

3. =
Summer
(July, August, and September)

4. =
Fall     

(October, November, and December)
For example, BRID1_T1W.131 contains Bridger Wilderness transmissometer data for the period January 1, 2013 through March 31, 2013.  The average size of a quarterly transmissometer file is 202 Kb.
SITE SPECIFIC NOTES FOR TRANSMISSOMETER DATA (1/1/2013 – 12/31/2013)
BRID1 – All readings from LPV-007 (installed 11/13/13 @ 1300 hrs) invalid. Bext too low and not matching actual conditions 11/13/13 – 12/31/13.
TRANSMISSOMETER SITE IN THE IMPROVE VISIBILITY MONITORING NETWORK (operated by USDA-FS):
BRID1 – Bridger Wilderness, WY  
